품 목 : 휴대용 페이즈 어레이 초음파 탐상기 모 델 : UT SOFTWARE Ultravision3 제조사 : ZETEC PC based 소프트웨어 윈도우 운영 체계 하에 있는 높은 사양의 데스크탑 뿐만 아니라 강력한 랩탑에서도 효율적으로 작동된다. 성능 계선을 위한 설계 Conventional UT 뿐만 아니라 광범위고 진보된 Phased Array UT 적용을 위해 설계되었다. 3D 작업환경 Phased array 탐촉자, 검사기법 개발, 검사 가능성 평가, 실질적 형상에서 데이터의 가시화 구현. 소프트웨어 개발 Kit (SDK) 소프트웨어 개발 키트는 고급 사용자들에게 그들만의 특징을 구현 할 수 있도록 한다. 믿을 수 있으며 안전한 소프트웨어 사용자의 올바른 접속관리, raw 데이터 보호

UT 초음파 탐상 검사 (Ultrasonic Testing)

경도엔터프라이즈(주) 경기도 성남시 중원구 상대원동 190-1 SKN 테크노파크 테크동 B114호

Tel　:　02-555-8181、Fax : 02-555-3171 , http://www.kdndt.com/

	UltraVision 3
	Basic	Advanced	3D
SETUP and ACQUISITION
Z-Scan UT, ZIRCON, DYNARAY Lite, TOPAZ	√	√	√
Basic self diagnostic with DYNARAY Lite	√	√	√
Automatic probe detection with the ZIRCON	√	√	√
DDF	√	√	√
Position dependant focal laws			√
Automatic PA calibration and TGC	√	√	√
Parameter access management(User Rights)	√	√	√
Operating logging (Log Viewer)	√	√	√
ADVANCED FOCAL LAW CALULATOR
Graphical feedback on focal law generation	√	√	√
Acoustic beam simulation		√	√
Focal law calulation on flat and cylindrical specimens	√	√	√
Support of complex geometries			√
1D and 2D flexible array and custom contoured wedges			√
SPECIMEN and OVERLAY MANAGEMENT
2D specimen overlay in Top, Side and End views	√	√	√
3D specimen(specimen generator, 3D overlay, Visualization)			√
Scanner creation tool			√
3D ray-tracing with postulated defects			√
TOFD
Calibration(flat and cylindrical) and processing (LW synchronization, LW removal, SAFT)	√	√	√
DATA FILES
Up to 20GB	√	√	√
ANALYSIS
Basic(measurement tools)and Advanded(indication table) analysis features	√	√	√
Volumetric Merge	√	√	√
3D Volumetric merge			√
Assisted Analysis		√	√
Off-line hysteresis(backlash) correction	√	√	√
Geometrical echo removal tool		√	√
Reporting feature	√	√	√
Retrieval and visualization of DAT,RDT,OPD and OUD file	√	√	√
Retrieval and visualization UVDATA and BEAMDATA file	√	√	√
ADDITIONAL
Multi-lanuage operation	√	√	√
Open architecture / software development kit (SDK)		√	√
Site License	√	√	√