품 목 : 탄성계수 측정장비 모 델 : RUSpec 제조사 : MAGNAFLUX 개 요 미국 MAGNAFLUX사에서 개발한 합금 탄성률 측정 장비로, 지금까지의 어떠한 방식(IE, NI, 4PB)의 장비와 차별화하여 쉽고, 빠른 측정으로 정확하고, 신뢰성 있는 데이터를 얻음으로써, 신소재에 대한 탄성 특성을 평가 할 수 있음. 특 징 복잡한 시험편 가공 없이 측정 가능 빠른 검사 속도 및 데이터 수집 능력 탄성계수, 전단 계수, 프와송비, 밀도등의 정보 수집 가능 신 공정 및 신 합금 개발 소재의 탄성 특성 평가

공명검사장비 (Process Compensated Resonant Testing)

경도엔터프라이즈(주) 경기도 성남시 중원구 상대원동 190-1 SKN 테크노파크 테크동 B114호

Tel　:　02-555-8181、Fax : 02-555-3171 , http://www.kdndt.com/

Features •. For isotropic materials, one set of measurements determines: √ Shear Modulus √ Young’s Modulus √ Bulk Modulus √ Poisson’s Ratio √ Density •Calculates all independent elastic constants with one set of measurements. for isotropic, cubic, hexagonal, tetragonal and orthorhombic structures •Provides extraordinary accuracy (capable of better than or equal to 0.1%) for large and small unflawed sample sizes •Rapidly determines elastic constants versus. temperature
RUSpec Measures •Resonant spectra for hard materials (metals, ceramics, and some composites) and calculates Elastic Constants (Cij) for rectangular parallelepipeds and cylinders •Samples from millimeters in size to greater than 10 centimeters •From liquid helium temperatures to temperatures in excess of 1850 °C (high and low temperature fixtures not provided)
RUSpec Products •RUSpec measurement system •RUSpec Software Suite Containing: √ RUSpec Data Acquisition Software √ RPModel Analysis for Rectangular Parallel- epipeds (RP) √ RPCyl Analysis for Cylinders √ RPR for calculating RP Solutions √ RPCYL for calculating Cyinder Solutions •Micro Nest (left) for small (< 2.5 cm samples) or a Universal Nest for larger samples
SYSTEM SETUP AND INITIAL INSPECTION CHECKS
Additional Connections
Non-US Power Connection

Power
전압 최대 전류 소비전력	115VAC±10%, 단상 3 Amps 350Watts
정밀도
측정 샘플의 순도에 따라 통상적으로 0.1%의 오차 범위를 갖음. 측정 샘플의 순도 및 형상에 따라 최대 0.01%의 오차 범위를 갖음.
주파수 범위
1 ㎑∼3㎒
온 도
작동 온도 설치 장소 온도	0∼45℃ -10℃∼60℃
습 도
0∼95%
컴퓨터 및 컨트롤러 사양
펜티움 Ⅳ＠2.8GHz 또는 40 Gigabyte 하드디스크와 512MB RAM(WINDOW XP이상)
Sample Holder
Precision type Universal type	2.5㎝보다 작은 sample 측정시 사용 5℃∼35℃에서 사용 0∼95%의 습도에서 사용 2.5㎝보다 큰 sample 측정시 사용 온도와 습도는 동일
측정 가능 물성
탄성계수, 전단계수, 프와송비 등 포함
측정 스테이지
XYZ 축으로 이동이 가능하며, 시편 고정을 위해 압력 게이지가 설치되어 있음.